Our device configurations

Below are the configurations for our RN2483 board, which might be handy to demonstrate demo applications. They can also be found on our thingsstack URL: <https://eu1.cloud.thethings.network/console/applications/lorahan/devices/eui-0004a30b001f2259>

const char\* AppKey = "C30F1715DFA6B9F21C2DCB07AC65FF00"

const char\* AppEUI = "0000000000000000"

const char\* DevEUI = "0004A30B001F2259"

**Formatter type:** ‘CayenneLPP’. When the decoder of different group is used, ‘Custom Javascript decoder’ needs to be chosen.

Afbeelding met tekst, schermopname, Lettertype, nummer

Automatisch gegenereerde beschrijving

Not specific to our device, but know this is needed as other configurations:

#include <TheThingsNetwork\_IOT.h>

#define LORA\_SERIAL Serial1

#define DEBUG\_SERIAL Serial

TheThingsNetwork ttn(LORA\_SERIAL, DEBUG\_SERIAL);